Controller: | FRITZ!WLAN USB Stick AC 430
Operating system: | Windows 10/8/7 x64 Editions
Version: | 06.20.10
Build: | 18.06.12

# Installation Information for the AVM FRITZ!WLAN USB Stick in Microsoft Windows 10/8/7 x64 Editions

NOTE | With this setup the FRITZ!WLAN USB Stick AC 430 can be installed in 64-bit Windows 10/8/7. If you have already installed the AVM FRITZ!WLAN USB Stick and only want to update the drivers, simply run the "SETUP.EXE" installation program. Then select the "Update" option.

## Contents

1. General Remarks

2. Installing the FRITZ!WLAN USB Stick

3. Updating Driver Software Previously Installed

4. Removing the FRITZ!WLAN USB Stick

5. Instructions for Optimum System Performance

## 1. General Remarks

Drivers developed especially for use in Windows 10/8/7 x64 Edition are supplied with your FRITZ!WLAN USB Stick. The true 64-bit device driver offers full support for all Microsoft Windows features, including Plug & Play and ACPI.

The FRITZ!WLAN USB Stick is a universal communications solution for WLANs. You should use the FRITZ!WLAN USB Stick with a pentium-class computer or notebook (500 MHz or higher). A free USB 2.0 or 3.0 slot must be available to connect the FRITZ!WLAN USB Stick.

The driver software for the FRITZ!WLAN USB Stick AC 430 supports the following WLAN standards:

- IEEE 802.11a (54 Mbit/s link rate)
- IEEE 802.11b (11 Mbit/s link rate)
- IEEE 802.11g (54 Mbit/s link rate)
- IEEE 802.11n (150 Mbit/s link rate)
- IEEE 802.11ac (433 Mbit/s link rate)
- security in accordance with IEEE 802.11i (WPA2), WPA, WEP (128/64)

The FRITZ!WLAN USB Stick can be used both in combination with AVM FRITZ!Box products and with any other WLAN devices that comply with the above standards. Find out which WLAN standards are provided by your WLAN remote site (router, other clients, etc.).

If you operate the FRITZ!WLAN USB Stick in combination with an AVM FRITZ!Box equipped with a USB host, you can use the AVM Stick & Surf technology. This makes WLAN configuration especially simple and secure.

The following components are installed with the FRITZ!WLAN USB Stick:

- complete driver software for WLAN operation
- the FRITZ!WLAN control software, developed by AVM
- system drivers for operation in combination with the Automatic WLAN Configuration

Note: During software updates the transmitter power of the FRITZ!WLAN USB Stick will be reset to the original value of 100%.

Back to top

## 2. Installing the AVM FRITZ!WLAN USB Stick

The AVM FRITZ!WLAN USB Stick is installed on your computer by means of a comprehensive installation routine. The installation comprises two basic steps:

- Connecting the FRITZ!WLAN USB Stick
- Installing the new hardware component and installation of the driver software for the FRITZ!WLAN USB Stick

### Connecting the FRITZ!WLAN USB Stick

Proceed as follows to install the FRITZ!WLAN USB Stick:

1. Install your AVM FRITZ!Box with WLAN support, your WLAN access point, or another WLAN client according to the supplied instructions.
2. If you are using an AVM FRITZ!Box with a USB host port, insert the FRITZ!WLAN USB Stick in the relevant port on the FRITZ!Box after launching FRITZ!Box operation. As soon as the "INFO" LED lights up, all of the parameters required for WLAN configuration are transmitted to the FRITZ!WLAN USB Stick (AVM Stick & Surf).
3. Connect the FRITZ!WLAN USB Stick with any USB port.

This concludes the connection of the FRITZ!WLAN USB Stick.

### Installing the Driver Software

The driver software for the FRITZ!WLAN USB Stick consists of the device driver and the WLAN control software FRITZ!WLAN. Both components are installed using the Windows "Add New Hardware Wizard".

### Installation in Windows 10/8/7 x64 Editions

1. Windows detects the FRITZ!WLAN USB Stick automatically. This process may take some time.
2. In the "Autoplay" dialog, select the "Run AVM FRITZ!WLAN USB Stick AC 430 Installation" option.
3. Then click "Continue" in the "User Account Control" dialog.
4. In the "Found New Hardware" window, select the option "Locate and install driver software (recommended)".
   If the "Program Compatibility Wizard" reports that the program may not have been installed correctly, click "Program was installed correctly." or "Cancel".
5. Then click "Continue" in the "User Account Control" dialog.
6. In the "Found New Hardware" dialog, select the option "I don't have disk. Show me other options.".
7. Then select "Browse my computer for driver software (advanced)" and enter the path to the driver software on your hard using the "Browse..." button.
   Attention: If you have downloaded a driver update file from the AVM Server, the archive extracts itself to the following location: "\PROGRAMS (x86)\AVM_UPDATE".
8. Click "Next" to install the driver software.
9. Conclude the installation by clicking "Close".

Once the installation has been concluded, you may establish a connection using the Microsoft WLAN service by clicking the network icon in the notification area.

### The FRITZ!WLAN Control Software

Right after the driver software is installed, the FRITZ!WLAN control software is installed automatically. If the FRITZ!WLAN control software was not configured on your computer, proceed as instructed in section 3 to install it later.

After FRITZ!WLAN USB Stick is connected to a WLAN remote site, FRITZ!WLAN appears as a program icon in the notification area of the task bar. If the WLAN connection is active, the program icon will be displayed in green. If there is no active WLAN connection, the program icon is gray. Double-click the control software icon FRITZ!WLAN in the notification area of the Windows taskbar to open the console. The console of the FRITZ!WLAN control software displays the FRITZ!WLAN USB Stick, the remote site and the connection between devices. Establishing connections with FRITZ!WLAN is always based on the same principle: search, find and connect.

The FRITZ!WLAN USB Stick and the FRITZ!WLAN control software are loaded automatically every time the system starts. Connections between the FRITZ!WLAN USB Stick and known WLAN access points are established automatically as long as a successful connection to this device has already been configured and the device is turned on. For details about the FRITZ!WLAN control software, see the manual accessible in the "Service / Manuals" area of the AVM home page.

Note: To connect to a wireless network use the Microsoft WLAN service.

Back to top

## 3. Updating Driver Software Previously Installed

To update driver software for FRITZ!WLAN USB Stick already installed on your system, proceed as follows:

1. Start the "SETUP.EXE" file from the driver update package. If you downloaded the update package from the AVM Data Call Center (ADC), this step is performed automatically when you extract the driver files to the folder "\Programs (x86)\AVM_update".
   Select the "Allow" button in the "User Account Control" dialog.
2. The installation program starts with a welcome dialog. Click "Continue".
3. From the next dialog, select the "Update" command and click "Continue".
4. Depending on the driver signature options set on your system you may be asked repeatedly whether you would like to cancel the installation because a driver is missing a signature. Ignore these messages and select "Install this driver software anyway" or "Continue Anyway" to continue installation.
   Ignore the Program Compatibility Wizard if Windows displays it, and select "Program was installed correctly".
5. Conclude the driver update by clicking the "Finish" button.
6. Now the FRITZ!WLAN software starts automatically.
7. Next, confirm the prompt to restart Windows or restart the computer manually.

Back to top

## 4. Removing the FRITZ!WLAN USB Stick

The FRITZ!WLAN USB Stick driver software and the FRITZ!WLAN control software are removed at the same time.
Proceed as follows:

1. Start the "SETUP.EXE" file from the driver update package. If you downloaded the update package from the AVM Server, this step is performed automatically when you extract the driver files to the "\Programs (x86)\AVM_update" folder.
   Select the "Allow" button in the "User Account Control" dialog.
2. Click "Continue" in the next window.
3. Select the "Removal" option.
4. Click "Finish" to complete the process of uninstalling the software.
5. Remove the FRITZ!WLAN USB Stick from the USB port on your computer.

This concludes the uninstallation of the FRITZ!WLAN USB Stick.

Back to top

## 5. Instructions for Optimum System Performance

If the chip set is recognized by Windows, it is recommende toupdate the Windows device drivers. Depending on the chip set used, the following driver sources are available:

- the newest Service Pack for your operation system
- install the chip set driver from the support or driver CD included with the system (see also the manual of the system or motherboard)
- load the chip set from the Internet:

- for INTEL systems: INTEL Application Accelerator Pack or the Chipset Software Installation Utility http://support.intel.com/support/
- for VIA systems: VIA Hyperion 4in1 www.viaarena.com
- for nForce systems: NVIDIA nForce drivers / Unified driver package www.nvidia.com

For more information on this topic and about additional chipset drivers, see http://www.babylonsounds.com/faq/kap11.html (unfortunately, only available in German).

For a maximum possible speed of 433 Mbit/s, the 802.11ac standard requires a connection encrypted using WPA2.

Have fun working with FRITZ!WLAN USB Stick in your WLAN!

AVM Berlin

Back to top

AZI 08/15